	OTM101  16:9 Open Frame Touch Monitor  

	7”~86” 16:9 Industrial Open Frame Touch Monitor
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	Key Features
· 7"~86" TFT  LCD display  
· PCAP  Touch
· 300nits Brightness，Upgradable to3500nits 
· 16:9 Ratio
· Embedded, Wall Mounted, Vesa 

	Display Parameters

	LCD Size
	10.1" TFT (LED Backlight)

	Resolution
	1280*800

	Brightness 
	1000cd/m² 

	Aspect ratio
	16:9

	Life Time
	50,000hrs

	Contrast Radio
	(500:1) 

	Response Time
	8ms

	Viewing Angle
	Whole View Angle 80/60(U/D), 80/80(L/R)

	Color Resolution
	16.7M

	Touch Screen Parameters

	Touch Type
	10 Points Capacitive Touch 

	Surface Hardness
	6H>(Capacitive Touch)

	Touch Validity:
	>1,000,000

	Resolution
	4096*4096

	Life Time
	50,000hrs

	Degree of protection

	Front Panel IP65
	Default

	Whole IP65
	Optional

	IO Interface

	DC
	DC 12V

	USB
	1x USB2.0 For Touch

	VGA
	1x 

	HDMI
	1x 

	Power Supply

	Power Supply
	12V DC Power Input

	Power Comsuption
	<30W

	Wide Voltage
	[image: 3b37a9b0-86dc-47ab-9b37-0892e718e732]Optional (DC 6~36V Wide Voltage, IPTS )

	Installation

	VESA
	100mm*100mm

	Embedded
	Cabinet Hole Size(Optional) 

	Environments

	Operating Temp
	-10℃~50℃

	Storage Temp
	-30℃~70℃

	Relative Humidity
	5~95%@10℃ (Non-condensing)

	Vibration
	5~500Hz,1.5G,0.15mm peak value

	Shake
	1.5 Grms, IEC 60068-2-64, 5 ~ 500 Hz, 1 hr/axis

	Shock
	10 Grems, IEC 60068-2-64, Half sine wave,for 11 ms

	EMC
	CE/FCC Class A

	Enclosure

	Housing Material
	Steel

	Dimensions
	396 mm (W) x 320 mm (D) x 50.5 mm (H)

	Net Weight
	1.5KG
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